SECTION 10 11 00 VISUAL DISPLAY SURFACES

PART 1	GENERAL

1.01 WORK INCLUDED

A. Provide the following items, as specified herein and indicated on the drawings:

1. Markerboards
2. Glass markerboards, magnetic.

1.02 RELATED SECTIONS

A. Projection Screens: 

B. Wood Blocking: 


1.03 REFERENCES

A. ASTM International

1. ASTM C1036 Specification for Flat Glass
2. ASTM C1048 Specification for Heat-Treated Flat Glass-Kind HS Coated and Uncoated Glass

B. ANSl - American National Standards Institute

1. ANSI Z-97.1 Safety Performance Specifications and Methods of Test Used in Buildings

1.04 SUBMITTALS

A. Samples: Submit samples of color finishes for all items specified for selection by Architect.

1. Submit 6" length sample of trim required.

B. Shop Drawings: Submit drawings showing sizes, arrangements, accessories and installation details of all items specified.

C. Submit manufacturer's product data showing reference numbers, construction details and methods of assembly.

D. Warranty
Job Name
GlasPro


10 11 00 - 1
VISUAL DISPLAY SURFACES

1. Markerboard: Provide written warranty to the Owner signed by an official of the manufacturer of the marker board stating that all marker boards which do not retain their original writing quality, original erasing quality and original visual acuity for 5 years after date of acceptance will be replaced without charge to the Owner.

E. Cleaning Instructions: Provide written instructions for any care, maintenance and cleaning required beyond normal custodial care.

F. Special Environmental Requirements: Submit the following in accordance with Section 01 81 13.

1. Adhesives shall have a VOC content of [50] <Insert value> g/L or less.
2. Product Data: For installation adhesives, indicating VOC content.
3. Laboratory Test Reports: For installation adhesives, indicating compliance with requirements for low-emitting materials.
4. Composite Wood Products: Products shall be made using ultra-low- emitting formaldehyde resins as defined in the California Air Resources Board's "Airborne Toxic Control Measure to Reduce Formaldehyde Emissions from Composite Wood Products" or shall be made with no added formaldehyde.
5. 	Laboratory Test Reports: For composite wood products, indicating compliance with requirements for low-emitting materials.


1.05 DELIVERY, STORAGE AND HANDLING

A. Deliver products in manufacturer's original unopened shipping cartons. Store indoors in clean, dry area in manner to prevent warping or physical damage.

B. Protect work from dust, dirt and physical damage during and after installation until final acceptance.

PART 2	PRODUCTS

2.01 MANUFACTURERS

A. GLASPRO; McNeill Bishop, m.bishop@glas-pro.com , Address: 9401 Ann Street, Santa Fe Springs, CA 90670-2613
Phone: Toll Free: 800-776-2368 | Local: 562-946-7722

2.02 REMARKABLE GLASS BY GLASPRO

A. Magnetic or non-magnetic: Magnetic Glassboard.

B. Surface type: Standard Low Iron Glass (Non-Ghosting Gloss).


	
	C.
	Custom Graphics?  No.

	
	D.
	Color Option: Standard White  .

	
	E.
  F.
 G.
	Sizes: Standard Sizes.
Mounting: Standoff.
Accessories: Marker Tray (Wall mounted).
· Additional details: Marker Tray (Wall mounted) 
Magnetic accessories: Marker Tray (Magnetic)
· Additional details: Marker Tray (Magnetic), Traysize: , .


	2.03
	
	MAGNETIC GLASS MARKERBOARD

	
	A.
	Manufacturers

	
	
	1. Basis of Design: Drawings and specifications are based on GLASPRO’S REMARKABLE GLASS.
2. Other Manufacturers: 

	
	B.
	Materials

	
	
	1. Description: Single sided magnetic/non-magnetic; polished edges, low iron tempered glass.
2. Sizes: As indicated on drawings.
3. Colors and Finish: As selected by Architect.
4. Thickness: 1/4” nominal.
5. Provide all required mounting devices for installation.

	2.04
	
	FABRICATION

	
	A.
	All glassboards shall be fully manufactured and assembled in the USA.

	PART
	3
	EXECUTION

	3.01
	
	INSPECTION

	
	A.
	Verify building items affecting this section are placed and ready to receive work.

	
	B.
	Field measurements shall be taken to verify that boards will fit in their designated locations.

	
	C.
	Install wood grounds or wood blocking as required.

	3.02
	



  A.




  B.
	INSTALLATION

Workmanship

1. Install boards straight and level and securely anchored in place.
2. Leave surfaces clean and free from defects at time of final acceptance.

Clean-up: Remove all cartons, debris, scraps, etc. and leave spaces clean and have boards ready for use.


	
	
	                                  
                                      END OF SECTION




